ZC-OPSH510 OPS PC Supports 10th 11th Gen Intel Core i3/i5/i7 CPU,2\*USB 3.0+4\*USB2.0,1\*Type C,1\*RJ45,

1\*OPS JAE Port,1\*HDMI+1\*DP,1\*Power Button,2\*Antennas,1\*Power LED,1\*HDD LED



**Main Features:**

1.) Intel LGA 1200 Socket,Supports 10th 11th Gen Intel Celeron/Pentium/Core i3/i5/i7

2.) Standard OPS Frame,the Size is 180\*195\*42mm

3.) Rich Storage,1\*M.2 NVME and 1\*SATA 2.5’’

4.) M.2 Slot for WIFI Module

5.) OPS JAE Support 4096x2304@60Hz

6.) Good Quality:All Solid Cap,With Stable and Reliable Performance

**ZC-OPSH510 OPS PC Specification**

|  |  |
| --- | --- |
| CPU | Intel LGA 1200 Socket  Support 10th 11th Intel Celeron/Pentium/Core i3/i5/i7 |
| Chipset | H510 |
| RAM | 2\*SO-DIMM DDR4,Max 64GB |
| Storage | 1\*SATA 2.5’’  1\*M.2 NVME/SATA |
| Graphics Card | CPU Integrated Intel UHD Graphics,Max Resolution 4096\*2304@60Hz |
| Display | OPS JAE 80Pins: 4096\*2304@60Hz HDMI 2.0 Signal  HDMI 1.4: 4096\*2304@30Hz  DP1.2: 4096\*2304@60Hz |
| Network Card | 1\*RTL8111E,Gigabit |
| WIFI | Optional |
| I/O Ports | 1\*DC Port  1\*HDMI  1\*DP  1\*OPS JAE Port  2\*USB 3.0  4\*USB 2.0  1\*USB Type C  1\*RJ45  1\*Power Button  1\*Power LED  1\*HDD LED  2\*WIFI Antenna |
| Size | 180\*195\*42mm |