**ZC-G52-ITX6412 Fanless Industrial PC Onboard Intel Elkhart Lake J6412 CPU 4 Cores 2.0GHz Burst to 2.6GHz Intel UHD**

**Graphics With 4\*USB 2.0,2\*USB 3.0,4\*RS232,2\*RS232/422/485,1\*VGA,1\*HDMI,2\*LAN Ports,1\*MIC,1\*SPK**



**Main Features:**

1) Onboard Intel Elkhart Lake J6412 4 Cores 2.0GHz Burst to 2.6GHz.

2) Intel Intel UHD Graphics Card,Support 4K

3) With 1\*VGA Ports,1\*HDMI,Support Double Display

4) Rich USB Ports,Support total 6\*USB Ports

5) Rich COM Ports,Support 4\*RS232+2\*RS232/422/485

6) Onboard 2\*Realtek RTL8111H Gigabit,Suppot PXE/Wake on LAN

7) Full aluminium alloy shell,dustproof,durable,resist compression

8) Fanless Design,Industrial Design,Best Quality,Cheap Price

9) mPCIE for WIFI/3G/4G module,1\*SIM Slot

**ZC-G52-ITX6412 Fanless Industrial Computer Specification**

|  |  |
| --- | --- |
| **CPU** | Intel Elkhart Lake J6412,4 Cores 2.0GHz Burst to 2.6GHz,TDP 10W |
| **RAM** | 1\*DDR4 SO-DIMM |
| **Storage** | 1\*M.2 Key M Support NVME/SATA SSD |
| 1\*2.5’’ Slot |
| **Graphics Card** | Intel UHD Graphics,Support 4K |
| **Network Card** | 2\*Realtek RTL8111H Gigabit |
| Support Wake On LAN,PXE |
| **I/O Ports** | 1\*VGA  1\*HDMI  4\*USB 2.0  2\*USB 3.0  1\*Audio Out  1\*MIC In  2\*RJ45  4\*RS232  2\*RS232/422/485  1\*DC Jack  1\*Power Button  2\*Antenna Holes |
| **Expand** | mPCIE for WIFI/3G/4G module  1\*Sim Slot |
| **Size** | 52\*215\*236mm |
| **Weight** | 1.85KG |
| **Power Supply** | DC12V |
| 9-36V (Optional) |
| **Working Temperature** | -10℃~+60℃ |
| **Storage Temperature** | -20℃~+70℃ |
| **Relative Humidity** | 5%-95% Relative humidity,no condensation |

